##### Martin Audio Blackline X115

The loudspeaker shall be a compact subwoofer consisting of one 15” reflex-loaded, long-excursion, low frequency transducer.

The on-axis frequency response shall be 45Hz-150kHz +/- 3dB and the loudspeaker shall produce a maximum SPL of 135dB peak calculated at 1 metre. Power handling shall be 500W AES, 2000W peak. Rated impedance shall be 8 ohms. The rear connector panel shall be fitted with three NL4 type connectors and the loudspeaker shall be operated in conjunction with a dedicated electronic controller.

The enclosure shall be made from plywood and finished with a black textured paint. Optional white and RAL colour finishes shall be available to special order. The enclosure shall be fitted with a pole-mount socket and M10 threaded inserts for eyebolt suspension. Provision shall be made for the fitment of castors and the drivers shall be protected by a perforated steel grille.

Dimensions (W x H x D) including feet shall be 465mm x 590mm x 565mm (18.3in x 23.2in x 22.2in). Weight shall be 27kg (59.5lbs).

The loudspeaker shall be the Martin Audio X115.