AD-P4T

The pendant-style 2-way co-axial system shall incorporate a 4.5-inch woofer with treated-paper cone and a 19 mm aluminum dome tweeter. The tweeter shall be mounted coaxially in front of the woofer on a waveguide that matches the directivity of the two drivers at the 1850 Hz crossover point.

The system shall meet the following performance criteria: conical coverage angle of 150 degrees; effective frequency range of 65 Hz to 20 kHz +0/-10 dB, measured on axis; broadband sensitivity of 87.9 dB (measured at 1 m with 4 V rms input); maximum continuous output of 102 dB SPL and maximum peak output of 108 dB SPL on axis at 1 meter; power handling of 30 watts for 8 hours with an IEC noise signal; recommended amplifier power of 60 watts; nominal impedance of 16 ohms.

The loudspeaker shall have a switchable low-distortion, wide-bandwidth laminated core transformer with taps for 30, 15, 7.5 and 3.8 watts at 70V and 30, 15 and 7.5 watts at 100V. The system shall be switchable between 16Ω (bypass) and constant-voltage operation.

The loudspeaker shall have an ABS enclosure. The baffle and the grille shall have either a white (RAL 9010) or black (RAL 9011) paintable finish with UV inhibitors to prevent discoloration. The enclosure shall retain the grille magnetically. Any logo on the grille shall be removable without leaving a blemish.

The loudspeaker enclosure shall have a steel hanger tab for support and shall include two 3.25 m quick-link 2 mm suspension cables with slip-lock fasteners. The loudspeaker connections shall be a locking 4-pole Euro-block that accepts two 12 AWG wire pairs.

The loudspeaker shall be listed as safe for use in air-handling spaces under UL1480. The loudspeaker shall meet or exceed IP-34 for ingress protection. The switchable transformer shall be listed under UL1876 and shall be CE and RoHS compliant. The baffle shall meet UL94-V0 and UL94-5VB flammability ratings and shall comply with IEC60849/EN60849 safety standards.

The loudspeaker's enclosure shall be 10.7 in (27.2 cm) high and 9.3 in (23.7 cm) in diameter. The loudspeaker shall weigh no more than 6.5 lb (2.9 kg).

The pendant-style 2-way co-axial system shall be the QSC AD-P4T.